08/01/2014

S407-14.docx

|  |
| --- |
| Use on projects when Double Course Chip Seal is to be measured by SQYD or m2. (Not needed if double chip seal measured by the ton) |

## Section 407. — CHIP SEAL

**Measurement**

**407.14** Add the following:

When double course chip seal (chip seal, type 2) is measured by the square yard (m2), measure the area only once. Chip seal, type 2 by the square yard (m2) includes both applications.