02/25/2025

Use on all projects.

## Section 106. — ACCEPTANCE OF WORK

**106.01 Conformity with Contract Requirements.** Add the following:

If the accuracy of Government test results is disputed, inform the CO. If the dispute is unresolved after reasonable steps are taken to resolve the dispute, further evaluation may be obtained by written request.

Where sample and testing procedures refer to AASHTO, ASTM, or other standards (designated as FLH T), use the procedure as modified in the FLH *Field Materials Manual*.

Where the specifications refer to AASHTO T 11, follow “Procedure B - Washing Using a Wetting Agent”.

Where the specifications refer to AASHTO T 310, follow the “Direct Transmission Method of In-Place Nuclear Density and Moisture Content”.

**106.03 Certification.** Delete the third paragraph and substitute the following:

See Table 106-3 for schedule for full or partial acceptance by material certification. Submit certification and sample of material for testing as required.

Check certifications before incorporating the material into the work to ensure that the requirements of the contract have been met. Mark the certifications with the following information: project number and name; pay item number and description; date; and Contractor-signed certification stating “to the best of our knowledge the materials certified by the attached certification represent the materials incorporated into the work of this contract”.

**Table 106-3**

**Schedule For Full or Partial Acceptance by Materials Certification**

| **Section** | **Description** | **Material** | **Material Property****Or Specification** | **Certification Frequency** | **Sample Frequency** |
| --- | --- | --- | --- | --- | --- |
| 302 | Crushed Aggregate | Crushed aggregate | Source, quality and gradation | 1 per source | 1 per source |
| 312 | Dust Palliative | Calcium chloridemagnesium chloride, lignosulfonate | As specified | 1 per shipment | First shipment |
| 403 | Asphalt Concrete | Aggregate asphalt mix | Source quality, gradation, stability, and grade | 1 per mix | 1 per source |
| 634 and 635 | Permanent Pavement Markings, Temporary Traffic Control | 634.02 as applicable, 635 as applicable | As specified | 1 per source | − |
| 701 | Cementitious Material | Portland cement, blended hydraulic cement, mortar cement | AASHTO M 85, M 240, ASTM C91 and ASTM C1392 as applicable | 1 per shipment | 1 per 100 tons |
| 702.01 | Asphalt Binder | Asphalt cement | AASHTO M 226 or M 320,  as applicable | 1 per shipment | 1 per shipment |
| 702.02 | Emulsified Asphalt | Emulsified asphalt | AASHTO M 140 or M 208 as applicable | 1 per shipment | 1 per shipment |
| 702.05 | Antistrip Additive | As specified | As applicable | 1 per shipment | − |
| 706 | Concrete Pipe | As specified | As applicable | 1 per shipment | − |
| 707 | Metal Pipe  | As specified | As applicable | 1 per shipment | − |
| 708 | Plastic Pipe | As specified | As applicable | 1 per shipment | − |
| 709 | Reinforcing Steel and Wire Rope | As specified | As applicable | 1 per shipment | For 709.01 submit 3, 1-yard bars of each size and grade of bar furnished.For 709.02 submit 1 6-foot length for each size furnished |
| 710 | Fencing and Mesh Fabrics | As specified | As applicable | 1 per shipment | − |
| 711 | Concrete Curing Material and Additives | As specified | As applicable | 1 per material source per material type | − |
| 712 | Joint Material | As specified | As applicable | 1 per shipment | − |
| 713 | Roadside Improvement Material | As specified | As applicable | 1 per shipment | − |
| 714 | Geosynthetic Material | As specified | As applicable | 1 per shipment | 1 per project per type |
| 715 | Piling | As specified | As applicable | 1 per shipment | − |
| 716 | Material for Timber Structures | Timber and hardware | As applicable | 1 per shipment | − |
| 717 | Structural Metal | As specified | As applicable | 1 per shipment | For 717.01(e) minimum 6 per shipment for each size used.For 717.091 per project |
| 718 | Traffic Signing and Marking Material | As specified | As applicable | 1 per shipment | − |
| 719 | Coating Material | As specified | As applicable | 1 per batch\lot | 1 sample for quantities> 25 gallons |
| 720 | Structural Wall and Stabilized Embankment Material | As specified | As applicable | 1 per shipment per material type | − |
| 721 | Electrical and Illumination Material | As specified | As applicable | 1 per shipment per material type | − |
| 722 | Anchor Material | As specified | As applicable | 1 per shipment per material type | − |
| 723 | Dampproofing and Waterproofing Material | Asphalt materials used for damproofing and waterproofing concrete and masonry surfaces | As specified for each type of asphalt material | 1 per shipment | − |
| 724 | Guardrail | As specified | As applicable | 1 per shipment | − |
| 725 | Miscellaneous Material | As specified | As applicable | 1 per shipment per material type | − |