02/25/2025

Include if the project has reinforced concrete retaining walls.

## Section 258. — REINFORCED CONCRETE RETAINING WALLS

**Measurement**

**258.08** Delete this Subsection and substitute the following:

When measuring retaining walls by the square foot, measure from gutter line at top of finished roadway to bottom of wall, excluding footings.

**Payment**

**258.09** Add the following:

Payment will be made under the reinforced concrete retaining wall pay item listed in the bid schedule which corresponds to the actual constructed height. For constructed wall heights that fall between two pay item heights, payment will be made under the pay item which most nearly describes the actual height. (For example, walls measuring 6.99 feet in height will be paid as a 6 foot wall, and walls measuring 7.00 feet in height will be paid as an 8 foot wall.)