02/25/2025

## Section 609. — CURB AND GUTTER

Include if project has existing asphalt gutters that will be overlaid.

**Construction Requirements**

**609.06 Asphalt Concrete Curb or Gutter.** Add the following:

Before overlaying existing asphalt gutters, clean and seal the cracks according to Section 414.

Include if project has asphalt gutter or asphalt curb.

**Measurement**

**609.11** Add the following:

When measuring asphalt gutters, measure the length along the face of the curb.

Do not measure the asphalt mixture included in asphalt curb or asphalt gutter.