02/25/2025

Include if the Contractor is required to construct a temporary stream diversion.

## Section 628. — TEMPORARY STREAM DIVERSIONS

**Construction Requirements**

**628.04 General.** Delete the first sentence and substitute the following:

Provide a stream diversion system for expected flow during in-water work activities that accommodates at least a <<<2-year>>> peak flood event of <<<350>>> cubic feet per second.

**628.05(d)** **Bypass pumping diversion.** Delete the third sentence and substitute the following:

Place a mesh screen over the intake with a maximum mesh size of 3/32 inch.