02/25/2025

## Section 635. — TEMPORARY TRAFFIC CONTROL

Include if the project has temporary construction signs.

**Construction Requirements**

**635.07 Construction Signs.** Add the following:

Provide the same type of sheeting on all post-mounted construction signs.

Include if temporary pavement markings are required.
Also include Standards 635-2 and 635-3 in the plans.

**635.14 Temporary Pavement Markings and Delineation.** Add the following to (c):

For seasonal suspensions, apply the permanent pavement marking pattern with temporary traffic paint.

Add the following after paragraph (c):

**(d) Delineation for unmarked pavements with vehicle positioning guides.** For unmarked pavements, install signs and vehicle positioning guides as shown in the plans.

Add the following to the last paragraph:

If permanent pavement markings are not placed within 14 days, provide, at no additional cost to the Government, additional temporary delineation equivalent to the permanent pavement marking pattern.

**Measurement**

**635.26** Add the following:

Include if the project has a temporary pavement marking pay item.

Do not measure temporary signs and raised pavement markers used for vehicle positioning guides installed according to Standard 635-3.

Include if the project has a flagger or TCS pay item.

Do not measure flagging or pilot car operations performed by the TCS.