02/25/2025

Include if using Section 501, 601, or 552 concrete.

## Section 701. — CEMENTITIOUS MATERIAL

**701.03 Pozzolans.** Delete Subsection (a) and substitute the following:

**(a) Fly ash.** Conform to AASHTO M 295 4.5 percent maximum

Class C or Class F.

When used to mitigate alkali-silica reactivity,

also available alkalis as equivalent Na2O