02/25/2025

Include if the Contractor is required to apply seed. Ask the partner agency for a specific seed mix to use.

*Example text:*

Use the following seed mix for all upland areas of disturbance:
Yarrow (Achillea millefolium) 2 pounds PLS/acre
Spike trisetum (Tristeum spicatum) 3 pounds PLS/acre
Wheeler's bluegrass (Poa wheeleri) 1 pound PLS/acre
Idaho Fescue (Festuca idahoensis) 4 pounds PLS/acre
Beaked Sedge (Carex rostrata) 1 pound PLS/acre
Lupine (Lupinus argentus) 1 pound PLS/acre

Total = 12 pounds PLS/acre

## Section 713. — ROADSIDE IMPROVEMENT MATERIAL

**713.04 Seed.** Add the following:

Use the following seed mix:

<<<Fill in project-specific seed mix>>>