*INCLUDE SECTION 414 ON ALL PROJECTS WITH 414 PAY ITEMS AND AS NEEDED BASED ON CLAUSE INSTRUCTIONS AND WHEN RECOMMENDED BY THE PAVEMENT REPORT/MEMO AND/OR BY THE MATERIALS ENGINEER. (IF USING LOS 414, ALSO INCLUDE LOS SECTION 712).*

$$414.00A

**Section 414. — ASPHALT PAVEMENT CRACK AND JOINT SEALING AND FILLING**

Revised 03 July 2024

*INCLUDE CLAUSE $$414.03A IF SPECIFYING THE WIDTH OF CRACKS NOT REQUIRING CLEANING - VERIFY WITH PAVEMENTS AND/OR MATERIALS ENGINEER IF CLAUSE IS APPROPRIATE TO USE. (IF USED, VERIFY/REVISE THE MAXIMUM WIDTH OF CRACKS THAT DO NOT REQUIRE CLEANING).*

$$414.03A

414.03. Add the following:

Do not clean cracks less than ½-inch wide.

*INCLUDE CLAUSE $$414.05A FOR CRACK SEALING AND FILLING.*

$$414.05A

414.05. Add the following:

Do not rout cracks unless directed by the CO.

*INCLUDE CLAUSE $$414.06A IF SPECIFYING THE WIDTH OF CRACKS NOT REQUIRING SEALING OR FILLING - VERIFY WITH PAVEMENTS AND/OR MATERIALS ENGINEER IF CLAUSE IS APPROPRIATE TO USE. (IF USED, VERIFY/REVISE THE MAXIMUM WIDTH OF CRACKS THAT DO NOT REQUIRE SEALING OR FILLING).*

$$414.06A

414.06. Add the following:

Do not seal or fill cracks less than ½-inch wide.