*INCLUDE SECTION 572 ON ALL PROJECTS WITH CONCRETE REPAIRS (THIS ALSO INCLUDES PROJECTS WITH WORK IN SECTIONS 553, 559, OR 570 IF APPLICABLE - VERIFY WITH BRIDGE)*

$$572.00A

**Section 572. — CONCRETE REPAIR**

Revised 20 May 2025

*INCLUDE THE FOLLOWING ON ALL PROJECTS WITH CONCRETE REPAIRS - VERIFY WITH BRIDGE IF CLAUSE IS APPROPRIATE TO USE - EDIT HAMMER IMPACT STRENGTH IF NECESSARY TO MEET PROJECT-SPECIFIC NEEDS*

##572.06A

572.06. Delete the second sentence of the first paragraph and substitute the following:

Use power-driven hand tools and other hand tools to remove existing concrete. Do not use jackhammers heavier than 30 pounds. Do not operate jackhammers and mechanical chipping tools at an angle more than 45 degrees measured from the surface of the concrete.