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Section 718. — TRAFFIC SIGNING AND MARKING MATERIAL
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INCLUDE THE FOLLOWING WHEN RETROREFLECTIVE SHEETING IS REQUIRED (TYPICALLY FOR 633 PERMANENT SIGN PANELS AND 635 TEMPORARY TRAFFIC CONTROL DEVICES)
$$718.01A
718.01.  Add the following:

For a list of acceptable manufacturers and products, refer to the FHWA, Traffic Sign Retroreflective Sheeting Identification Guide found at https://highways.dot.gov/safety/other/visibility/2014-traffic-sign-retroreflective-sheeting-identification-guide.

INCLUDE THE FOLLOWING ON ALL PROJECTS WITH RECTANGULAR RAPID-FLASHING BEACON (RRFB) SYSTEM. (IF USED, ALSO NCLUDE CLAUSE $$636.02)
$$718.04A
Add the following after Subsection 718.04:

718.04A  Sign Support for Rectangular Rapid-Flashing Beacon Systems.  Provide sign supports that meet MASH criteria and conform to Task Force 13 (TF13), Guide to Standardized Roadside Hardware.

INCLUDE THE FOLLOWING ON ALL PROJECTS WITH WATERBORNE PAVEMENT MARKINGS (TYPICALLY TYPE B OR TYPE C PAVEMENT MARKINGS)
$$718.09A
718.09.  Delete Subsections (a), (b) and (i).

INCLUDE THE FOLLOWING ON ALL PROJECTS WITH RECTANGULAR RAPID-FLASHING BEACON (RRFB) SYSTEMS. (IF USED, ALSO NCLUDE CLAUSE $$636.02)
$$718.19A.
Add the following after Subsection 718.18:

718.19  Rectangular Rapid-Flashing Beacon Systems.  Provide rectangular rapid-flashing beacon (RRFB) light bars with black housing.

Provide solar panels, batteries, and solar engines capable of operating under ambient temperature conditions from -30 °F to 150 °F and supporting a minimum of 1,000 daily activations.

Provide solar engines with a natural finish.

Provide corrosion resistant (weathering) steel posts.





