## Section 617. — GUARDRAIL

07/01/24–FP14

WFL Specification 11/12/20 6170010

Include the following when weathering agent is required on galvanized steel guardrail components.

Material

### 617.02

Add the following:

Painting 563

Construction Requirements

WFL Specification 07/01/24 6170015

Include the following when using guardrail terminal systems. Consult with Safety.

### 617.03 General.

Add the following:

Furnish [INSERT flared OR tangent] terminals meeting [INSERT MASH or NCHRP 350] Test Level [INSERT Test Level].

WFL Specification11/12/20 6170020

Include the following when weathering agent is required on galvanized steel guardrail components.

Add the following:

Apply weathering agent to all galvanized steel guardrail system and terminal section components according to Section 563.

WFL Specification 07/01/24 6170030

Include the following on all projects where work is required under this section.

### 617.04 Post Installation.

Amend as follows:

Delete the third paragraph and substitute the following:

Complete adjacent earthwork, aggregate placement and other roadway surfaces to line and grade as applicable before installation of guardrail posts. Do not damage adjacent pavement, subsurface utilities, or drainage features during post installation.

WFL Specification 08/01/14 6170040

Include the following when alternate hole arrangements are required.

Note: Use for future pavement overlays. Insert 617-10 for wood posts and 617-11 for steel posts.

Add the following:

Use alternate hole arrangement detail as shown on Standard 617-[INSERT #].

WFL Specification 11/12/20 617050

Include the following when weathering agent is required on galvanized steel guardrail components.

### 617.11 Acceptance.

Add the following:

Painting will be evaluated under Section 563.