## Section 634. — PERMANENT PAVEMENT MARKINGS

04/02/21–FP14

Measurement

WFL Specification 04/02/21 6340010

Include the following when work is required under this Section.

### 634.12

Add the following to the second paragraph:

When two coats of paint are required, measure each coat.