## Section 310. — COLD IN-PLACE RECYCLED ASPHALT BASE COURSE

01 APR 2024 – FP-24

WFL Specification 01 APR 2024 3100010

Include the following when work is required in this Section.

Material

### 310.10 Construction Joints.

Delete Subsection (a) and substitute the following:

**(a) Longitudinal joints.** Offset the longitudinal joint of one layer at least 6 inches) from the joint in the layer immediately below. Make the longitudinal joint in the top layer along the striped centerline of two-lane roadways or at the lane lines of roadways with more than two lanes.