## Section 554. — REINFORCING STEEL

01 APR 2025 – FP-24

Construction Requirements

WFL Specification 01 APR 2025 5540010

Include the following when work is required in this Section.

**554.08 Placing and Fastening**. Delete the fourth sentence of the fourth paragraph and substitute the following:

Place reinforcing steel in deck slabs within plus ¼ inch of the vertical plan location.