## Section 617. — GUARDRAIL

01 APR 2024 – FP-24

WFL Specification 01 APR 2024 617010

Include the following when adding SCRs to this Subsection.

Construction Requirements

### 617.04 General.

WFL Specification 01 APR 2024 6170020

Include the following when using guardrail terminal systems. Consult with Safety for fill-ins.

Note: Duplicate as needed for projects with multiple requirements.

Add the following:

Use [INSERT flared or tangent] terminals meeting [INSERT MASH or NCHRP 350] Test Level [INSERT TEST LEVEL].

WFL Specification 01 APR 2024 6170030

Include the following when using crash cushions. Consult with Safety for fill-ins.

Add the following:

Use crash cushions meeting [INSERT MASH or NCHRP 350] Test Level [INSERT TEST LEVEL].

WFL Specification 01 APR 2024 6170040

Include the following when weathering agent is required on galvanized steel guardrail components.

Add the following:

Apply weathering agent to all galvanized steel guardrail system and terminal system components according to Section 563.

WFL Specification 01 APR 2024 6170050

Include the following when alternate hole arrangements are required.

Note: Use for future pavement overlays. Insert 617-10 for wood posts and 617-11 for steel posts.

### 617.05 Post Installation.

Add the following after the fifth paragraph:

Use alternate hole arrangement detail as shown on Standard 617-[INSERT #].

WFL Specification 01 APR 2024 617060

Include the following when weathering agent is required on galvanized steel guardrail components.

### 617.11 Acceptance.

Add the following:

Coating will be evaluated under Section 563.