## Section 625. — TURF ESTABLISHMENT

01 APR 2024 – FP-24

Construction Requirements

WFL Specification 01 APR 2024 6250010

Include the following when work is required under this Section.

### 625.03 General.

Delete this Subsection and substitute the following:

Apply turf establishment to finished slopes and ditches between [INSERT DATE] and [INSERT DATE]. Do not apply turf establishment during windy weather or when the ground is excessively wet, frozen, snow covered, extremely dry, cloddy, hard pan, or not friable.

WFL Specification 01 APR 2024 6250030

Include the following when water is not required.

Note: If water is required include pay item in EE.

### 625.05 Watering.

Delete this Subsection.

WFL Specification 01 APR 2024 6250040

Include the following when fertilizing by hydraulic method is required.

### 625.06 Fertilizing.

Add the following to Subsection (b):

Apply fertilizer at the rate of [INSERT #] pounds per slurry unit. Fertilize areas inaccessible to hydraulic-type equipment by hand.

WFL Specification 01 APR 2024 6250050

Include the following when seeding by hydraulic method is required.

Note: List seed mix in Subsection 713.04.

### 625.07 Seeding.

Add the following to Subsection (b):

Apply the seed at the rate of [INSERT #] pounds of live seed per [INSERT ACRE or SLURRY UNIT].

WFL Specification 01 APR 2024 6250060

Include the following when mulching by hydraulic method is required.

Note: add alternative mulches if acceptable.

### 625.08 Mulching.

Delete the second and third paragraphs of Subsection (b) and substitute the following:

Apply [INSERT MULCH DESCRIPTION] at a rate of [INSERT #] pounds per [INSERT ACRE OR SLURRY UNIT] upon completion of seeding and fertilizing applications. This rate does not apply to mulch for tracer applied under Subsection 625.07(b), Seeding, Hydraulic Method.