## Section 628. — TEMPORARY STREAM DIVERSIONS

01 JUL 2024– FP-24

WFL Specification 01 JUL 2024 6280010

Include the following on projects that require temporary stream diversions.

### 628.05(d) Bypass pumping diversion. Delete the third sentence and substitute the following:

Place a mesh screen over the intake with a maximum mesh size of 3/32 inch.