## Section 635. — TEMPORARY TRAFFIC CONTROL

01 APR 2025 – FP-24

Construction Requirements

WFL Specification 01 APR 2024 6350010

Include the following when using crash cushions or when impact attenuators are required. Consult with Safety for fill-ins.

### 635.04 General.

Add the following:

Use crash cushions or impact attenuators meeting [INSERT MASH or NCHRP 350] Test Level [INSERT TEST LEVEL].

WFL Specification 01 APR 2024 6350020

Include the following when work is required under this Section.

### 635.07 Construction Signs.

Delete this Subsection and substitute the following:

**Construction Signs.** Roll-up signs may be used instead of panels when approved.

Furnish posts conforming to Subsection 718.04, except wood posts may be untreated. Install posts according to Subsection 633.04. Portable sign supports may be used instead of sign posts when approved.

Remove or completely cover unnecessary signs.

WFL Specification 01 APR 2024 6350030

Include the following when automated flagger assistance devices (AFADs) may be used.

### 635.10 Flaggers.

Add the following:

Flaggers may operate automated flagger assistance devices (AFADs) when approved. Use AFADs according to the MUTCD.

WFL Specification 01 APR 2024 6350040

Include the following on all projects.

### 635.12 Portable Traffic Barriers.

Add the following:

Temporary steel barrier may be used when approved.

WFL Specification 01 APR 2024 6350050

Include the following when temporary pavement markings and delineation is required on the final alignment before permanent markings are applied. Not appropriate for use when project staging requires interim markings that are different than those needed for the final alignment.

 Note: Use when paving will last more than one day.

### 635.14 Temporary Pavement Markings and Delineation.

Add the following after the second paragraph:

Place temporary pavement markings to the same locations and cycle lengths as shown in the plans for permanent pavement markings, including all passing zones.

WFL Specification 01 APR 2025 6350060

Include the following when work is required under this Section.

### 635.25 Acceptance.

Delete the first paragraph and substitute the following:

**Acceptance.** Material for temporary traffic control devices will be evaluated under Subsections 106.02 and 106.03. Do not provide a copy of the certifications for temporary traffic control materials to the CO, unless otherwise directed.

WFL Specification 01 APR 2025 6350070

Include the following when the Traffic Control Supervisor is a pay item measured by the DAY in the Bid Schedule.

Measurement

### 635.26

Add the following:

Measure Traffic Control Supervisor by the day for the work described in Subsection 156.09.

A day will be measured when:

**(a)** Construction operations require a Traffic Control Supervisor during the normal working days;

**(b)** The Traffic Control Supervisor makes normal checks during nonwork hours; or

**(c)** The Traffic Control Supervisor is called out during nonwork hours.

Do not measure flagging performed by the Traffic Control Supervisor when there is a pay item in the bid schedule for Traffic Control Supervisor.

WFL Specification 01 APR 2024 6350080

Include the following when temporary pavement markings are required.

Add the following:

Do not measure temporary signs and pavement markers substituted for temporary pavement markings according to Subsection 635.14.