## Section 725. — MISCELLANEOUS MATERIAL

01 NOV 2024 – FP-24

WFL Specifications 01 NOV 2024 725005

Include the following when Stabilized Aggregate Surface Course (Section 311) is required.

**725.02(b) Calcium chloride flake**.

Delete this Subsection and substitute the following:

**(b) Calcium chloride solid.** Conform to ASTM D98, Type S, Grade N4, Type A or B.

WFL Specification 01 JUL 2024 725110

Include the following when weathering agent is required.

### 725.21 Weathering Agent.

(Added Subsection).

Furnish a weathering agent that colors the specified surfaces to a brownish earth tone, contains no pigments and conforms to the following:

**(a)** A soluble solution that contains organic acids and natural oxidizers.

**(b)** All coloring developed through a reactionary process that etches surfaces, producing a finish that’s resistant to fading from exposure to sunlight, with an expected performance life exceeding 10 years in nonaggressive climates.

**(c)** An environmentally benign product when used according to the manufacturer’s recommendations.

WFL Specification 01 APR 2024 725120

Include the following when weathering agent is applied to galvanized steel.

**(d)** A product that causes negligible zinc coating losses when applied to galvanized surfaces.

Natina® Steel is an acceptable product for coloring galvanized surfaces.

Natina® Steel

manufactured by Natina Products, LLC

1577 First Street

Coachella, CA 92236 USA

(877) 762-8462

[www.natinaproducts.com](http://www.natinaproducts.com/)

WFL Specification 01 APR 2024 725130

Include the following when weathering agent is applied to rock.

PermeonTM and Natina® Rock are acceptable products for coloring rock surfaces.

Natina® Rock PermeonTM

manufactured by Natina Products, LLC manufacturered by Soil Tech

1577 First Street 6420 South Cameron, Suite 207

Coachella, CA 92236 USA Las Vegas, NV 89118

(877) 762-8462 (702) 873-2023

[www.natinaproducts.com](http://www.natinaproducts.com/) [www.soil-tech.com](http://www.soil-tech.com)

WFL Specification 01 APR 2024 725140

Include the following when weathering agent is applied to cementicious surfaces.

PermeonTM and Natina® Concrete are acceptable products for coloring cementicious surfaces.

Natina® Concrete PermeonTM

manufactured by Natina Products, LLC manufacturered by Soil Tech

1577 First Street 6420 South Cameron, Suite 207

Coachella, CA 92236 USA Las Vegas, NV 89118

(877) 762-8462 (702) 873-2023

[www.natinaproducts.com](http://www.natinaproducts.com/) [www.soil-tech.com](http://www.soil-tech.com)