08/01/2014

S706-14.docx

|  |
| --- |
| Include subsections below as appropriate. |

## Section 706. — CONCRETE PIPE

|  |
| --- |
| Include the following when precast concrete box culverts are allowed: |

**706.07 Precast Reinforced Concrete Box Sections.** Add the following:

Concrete aggregates shall conform to subsections 703.01(b) and 703.02(c) for Alkali-silica reactivity.