02/25/2025

Include if using a double course chip seal pay item measured by SQYD (not needed if double chip seal measured by the ton).

## Section 407. — CHIP SEAL

**Measurement**

**407.14** Add the following:

When double course chip seal (chip seal, type 2) is measured by the square yard, measure the area only once. Chip seal, type 2 by the square yard includes both applications.