02/25/2025

Include if integral color is required in structural concrete. Generally structural concrete is required for bridges, culverts, walls, and foundations (items that require load analysis or “that you can drive on”).

Insert the description of the concrete to be colored and the color number in the spaces provided below.

## Section 552. — STRUCTURAL CONCRETE

**552.14 Finishing Formed and Deck Concrete Surfaces.** Add the following:

**(h) Class 8 - Integral color finish.** Provide integral color for all concrete in the <<<describe>>> by adding a concrete coloring agent. Match the color AMS-STD-<<<fill in number>>> in AMS Standard 595A for the colored concrete (after curing).