02/25/2025

Include if steel structures are required.

## Section 555. — STEEL STRUCTURES

**Construction Requirements**

The AISC Quality Certification Program identifies categories related to bridge fabrication. Insert the applicable category. Coordinate with the Bridge Engineer.

**555.07 Fabrication.** Delete the first sentence of the first paragraph and substitute the following:

Fabricate the structural steel in a fabricating plant that is <<<Certified Bridge Fabricator-Simple (SBR), Certified Bridge Fabricator-Intermediate (IBR) OR Certified Bridge Fabricator-Advanced (ABR) with supplemental program requirements for: Applicators of Complex Coatings Endorsement (CCE) or Fracture Control Endorsement (FCE)>>>, under the AISC, *Quality Certification Program*.

The AISC Quality Certification Program identifies categories related to bridge erection. Insert the applicable category. Coordinate with the Bridge Engineer.

**555.18 Erection.** Delete the third sentence of the first paragraph and substitute the following:

Use steel erector certified under the Certification Program for Erectors (CSE) with <<<Seismic Endorsement, Metal Deck Endorsement, or Bridge Endorsement>>> under the AISC, *Quality Certification Program*.