02/25/2025

Include if project has rumble or mumble strips.

## Section 633. — PERMANENT TRAFFIC CONTROL

**Construction Requirements**

**633.07 Rumble and Mumble Strips.** Add the following:

Provide equipment capable of milling concave indentations with a vacuum attachment to remove the residue from the roadway.