*INCLUDE SECTION 104 ON ALL PROJECTS WITH CLAUSE $$104.03A AS A MINIMUM*

$$104.00A

Section 104. — CONTROL OF WORK

Revised 22 June 2016

*INCLUDE THE FOLLOWING ON ALL PROJECTS*

$$104.03A

104.03(c). Delete the first sentence of the first paragraph and substitute the following:

Furnish one full-size (24-inch by 36-inch) paper copy of the plans from the Government-provided electronic plans, and use this set of plans exclusively for as-built drawings.

*INCLUDE THE FOLLOWING ON NPS PROJECTS (IF INCLUDING FOR OTHER PARTNERS, MAKE APPROPRIATE EDITS)*

$$104.05A

104.05. Add the following:

When hauling on National Park Service roads, do not exceed the load restrictions shown in Table 104-1.

|  |
| --- |
| **Table 104-1****Load Restrictions** |
| **Single Units** | **Gross Vehicle Weight, pounds** |
| 2 axles | 40,000 |
| 3 axles | 48,000 |
| 4 or more axles | 52,000 |
| **Combination Units** | **Gross Vehicle Weight, pounds** |
| 3 axles | 57,000 |
| 4 axles | 62,000 |
| 5 or more axles | 66,000 |

Where the ground is saturated with water or during periods of freezing and thawing, the CO may impose further load restrictions or suspend hauling.

*INCLUDE THE FOLLOWING, IF APPROPRIATE (IF $$104.05A IS INCLUDED, DO NOT INCLUDE $$104.05B INSTRUCTION LINE)*

$$104.05B

104.05. Add the following:

Operate loaded vehicles hauling material at speeds not exceeding 40 miles per hour or the posted speed limit, whichever is lower, and spaced at 500-foot minimum intervals. When hauling on bridges, do not exceed 25 miles per hour or the posted speed limit, whichever is lower, or operate more than 1 loaded hauling vehicle at a time.

*INCLUDE THE FOLLOWING IF HAULING MATERIALS INTO THE PROJECT (IF $$104.05A AND/OR $$104.05B ARE INCLUDED, DO NOT INCLUDE $$104.05C INSTRUCTION LINE)*

$$104.05C

104.05. Add the following:

Hauling will only be permitted from the nearest point of public access to the work site. Minimize hauling over completed pavement.

*INCLUDE THE FOLLOWING IF RESTRICTING ACCESS TO THE PROJECT THROUGH A SPECIFIC ROADWAY (IF $$104.05A, $$104.05B, AND/OR $$104.05C ARE INCLUDED, DO NOT INCLUDE $$104.05D INSTRUCTION LINE)*

$$104.05D

104.05. Add the following:

Do not use *(insert roadway name)* to access the project site during construction.