*INCLUDE SECTION 712 AS NEEDED BASED ON CLAUSE INSTRUCTIONS*

$$712.00A

**Section 712. — JOINT MATERIAL**

Revised 28 September 2017

*INCLUDE THE FOLLOWING FOR CRACK FILLER MATERIAL (INCLUDE FOR ALL PROJECTS WITH 414 CRACK FILLING PAY ITEMS) (IF USED, ALSO INCLUDE CLAUSES $$414.05A, $$414.06A AND $$414.06C)*

$$712.01A

712.01(a)(2). Delete the Subsection and substitute the following:

**(2)** Crack filler, hot-applied, pourable, aggregate filled, ASTM D5078

polymer modified mastic for concrete and asphalt

concrete pavements