*INCLUDE SECTION 301 ON ALL PROJECTS WITH 301 AGGREGATE PAY ITEMS*

$$301.00A

Section 301. — UNTREATED AGGREGATE COURSES

Revised 30 August 2024

*INCLUDE CLAUSES $$301.03A AND $$301.03B ON ALL PROJECTS WITH 301 AGGREGATE PAY ITEMS*

*WHEN USING CLAUSE $$301.03A, ALSO INCLUDE CLAUSE $$154.03A*

$$301.03A

301.03. Add the following to the second paragraph:

Submit the representative 300-pound sample to the EFLHD Central Laboratory in Sevierville, Tennessee at the address shown in Subsection 154.03.

*WHEN USING CLAUSE $$301.03B, ALSO INCLUDE CLAUSE $$703.05F, AND THE FOLLOWING:*

* *FOR PROJECTS WITH AGGREGATE BASE, INCLUDE CLAUSE $$703.05C.*
* *FOR PROJECTS WITH SURFACE COURSE AGGREGATE, INCLUDE CLAUSE $$703.05E.*

*SEE SUBSECTION 703.05 CLAUSES FOR ADDITIONAL INSTRUCTIONS FOR EACH TYPE OF 301 AGGREGATE PAY ITEM*

$$301.03B

301.03. Add the following:

An alternate state department of transportation aggregate gradation that is produced according to Subsection 703.05 may be submitted for approval. Provide target values within the allowable target value range of the state department of transportation aggregate gradation. When target values are not provided, the preproduction target values will be the midpoint of the allowable target value range of the state department of transportation aggregate gradation. The allowable deviation (±) from the target values will be according to Table 703-2A.

The maximum allowable pay factor under Subsection 301.10 for a state department of transportation aggregate gradation will be 1.00.