*INCLUDE SECTION 712 AS NEEDED BASED ON CLAUSE INSTRUCTIONS*

$$712.00A

**Section 712. — JOINT MATERIAL**

Revised 30 August 2024

*INCLUDE THE FOLLOWING WHEN CRACK FILLING IS REQUIRED (TYPICALLY FOR PROJECTS WITH 414 CRACK FILLING PAY ITEMS) (IF USING THIS CLAUSE, ALSO INCLUDE LOS SECTION 414).*

$$712.01A

712.01(a)(2). Delete the Subsection and substitute the following:

**(2)** Crack filler, hot-applied, pourable, aggregate filled, ASTM D5078

polymer modified mastic for concrete and asphalt

concrete pavements