## Section 710. — FENCE AND GUARDRAIL

7/19/19–FP14

WFL Specification 07/19/19 7100010

Include the following when using steel-backed timber guardrail.

### 710.06(d) Steel-backed log rail.

Delete the second paragraph and substitute the following:

Fabricate Steel backing elements according to ASTM A242.