## Section 105. — CONTROL OF MATERIAL

04/02/21– FP-14

WFL Specification 08/01/14 1050010

Include the following in all projects.

### 105.02 Material Sources.

Amend as follows:

WFL Specification 08/01/14 1050020

Include the following on projects when there are no Government-provided sources.

**(a) Government-provided sources.**

Delete the text of this Subsection and substitute the following:

There are no Government-provided sources for this project.

WFL Specification 04/20/18 1050030

Include the following when Government-provided sources are available.

Do not list material sources as Government-provided sources unless both quality and quantity can be assured. Coordinate with WFL Materials and Geotechnical.

**(a) Government-provided sources.**

Delete the last paragraph and substitute the following:

The quality of material is generally acceptable. Variations in quality should be expected as it is not feasible to ascertain the quality of material for an entire deposit from exploratory samples. Determine the quantity, type of equipment, and work necessary and produce acceptable material to be incorporated into the work.

Aggregate source quality tests as shown in the Sampling, Testing, and Acceptance Requirements table of the other Sections are not required. If aggregate source quality tests are performed, follow the requirements of the Sampling, Testing, and Acceptance Requirements tables. Allow the CO the opportunity to witness sampling and splitting of test material.

Perform quality control sampling and testing according to the approved Contractor Quality Control Plan in Section 153 and the applicable Sampling, Testing, and Acceptance Requirements tables included at the end of each Section. Allow the CO the opportunity to witness sampling and splitting of test material.

WFL Specification 08/01/14 1050040

Include the following when Government–provided sources are available, and edit as needed.

* List material, Section work done under, and material source No./Name.
* List estimated quantity available from the material source
* Include GPS coordinates if available.

Coordinate with WFL Materials and Geotechnical.

Government-provided sources for this project are identified as follows:

* Government-provided optional sources.

Obtain material for use as [INSERT BORROW / RIPRAP / BOULDERS / ETC.] and in the production of aggregates under [INSERT 301 / 302 / 401 / ETC.] from [INSERT MATERIAL SOURCE NO. OR NAME].

[INSERT MATERIAL SOURCE NO. OR NAME] is estimated to contain [ENTER QUANTITY] of material.

[INSERT MATERIAL SOURCE NO. OR NAME] is a [INSERT GRAVEL DEPOSIT OR QUARRY] located on [INSERT OWNER] land in Section [INSERT #], T [INSERT #], R [INSERT #], [INSERT MERIDIAN], as shown on the plans. Approximate Global Positioning System (GPS) coordinates for the source are [INSERT COORDINATES].

* Government-provided mandatory sources.

Obtain material for use as [INSERT BORROW / RIPRAP / BOULDERS / ETC.] and in the production of aggregates under [INSERT 301 / 302 / 401 / ETC.] from [INSERT MATERIAL SOURCE NO. OR NAME].

[INSERT MATERIAL SOURCE NO. OR NAME] is estimated to contain [ENTER QUANTITY] of material.

[INSERT MATERIAL SOURCE NO. OR NAME] is a [INSERT GRAVEL DEPOSIT OR QUARRY] located on [INSERT OWNER] land in Section [INSERT #], T [INSERT #], R [INSERT #], [INSERT MERIDIAN], as shown on the plans. Approximate Global Positioning System (GPS) coordinates for the source are [INSERT COORDINATES].

WFL Specification 08/01/14 1050050

Include the following when conditions for use will be required by the material source owner. Edit as required.

Meet the following conditions for material obtained from [INSERT MATERIAL SOURCE NO. OR NAME]:

* [INSERT CONDITIONS].
* [INSERT CONDITIONS].
* [INSERT CONDITIONS].

WFL Specification 01/01/14 1050060

Include the following in projects that meet both of the following requirements:

When government provided sources are available, and;

When there is no charge for material taken from the source.

There is no charge for material taken from [INSERT MATERIAL SOURCE NO. OR NAME].

WFL Specification 01/01/14 1050070

Include the following in projects that meet both of the following requirements:

When government provided sources are available, and;

When there is a charge for material taken from the source.

Pay [INSERT PERSON, COMPANY, OR AGENCY] a royalty of [INSERT $$ AMOUNT] per cubic [INSERT YARD OR METER], or if the material is weighed, [INSERT $$ AMOUNT] per [INSERT TON OR METRIC TON] for material furnished from this source and incorporated into the work.

Make monthly royalty payments directly to:

[INSERT OWNER OF THE SOURCE AND ADDRESS]

WFL Specification 09/17/18 1050080

Include the following on all projects that the Government does not provide materials.

**(b) Government-provided material stockpile.**

Add the following:

There are no Government-provided material stockpiles for this project.

WFL Specification 04/20/18 1050090

Include the following on all projects that the Government provides material. Describe the type of material (seed, culvert pipe, crushed rock, etc.), the work to be constructed (turf establishment, drainage structures, untreated aggregate courses, etc.), where the material is located, and how to arrange for obtaining the material (contact info).

**(b) Government-provided material stockpile.**

Add the following:

The Government will furnish [DESCRIBE MATERIAL] for use in [DESCRIBE WORK or SECTION TITLE]. The material is available [DESCRIBE LOCATION AND HOW TO OBTAIN MATERIAL].

WFL Specification 04/02/21 1050100

Include the following on all projects.

**(c) Contractor-located sources.**

Delete the text of this Subsection and substitute the following:

The Contractor is responsible for Contractor-located material sources, including established commercial material sources. Use sources that fulfill the contract quantity and quality requirements. Determine the quantity, type of equipment, and work necessary to select and produce an acceptable material. Secure permits and clearances for use of the source and submit copies of the documents to the CO. Follow the environmental requirements of Subsection 107.10(d) and anticipate a minimum of 60 days for approvals for use of any contractor located site or source. Submit available historical data indicating acceptable material can be produced from the source. Perform quality control sampling and testing according to the approved Contractor Quality Control Plan in Section 153, aggregate source quality tests, and applicable Sampling, Testing, and Acceptance Requirements table included at the end of each Section. Allow the CO the opportunity to witness sampling and splitting of the test material.

WFL Specification 04/02/21 1050110

Include the following on all projects when required by the partner agency.

Note: Coordinate with partner agencies on specific requirements and edit as required.

**Weed free certification.** All material sources and materials incorporated into the work must be certified to be free from noxious weeds, invasive plants, and other deleterious materials by a federal, state or local public agency. Commercial certifications may be acceptable if materials have been certified through the North American Weed Free Forage Program standard or a similarly recognized certification process approved by the CO. Submit material certifications to the CO for approval at least 7 days before their use in the work.

WFL Specification 01/01/14 1050120

Include the following when TERO for materials sources is required. (Except for Glacier National Park projects) Edit as required.

Materials obtained from within the boundaries of the [INSERT TRIBAL JURISDICTION] may be subject to the [INSERT TRIBE NAME] Tribal Employment Rights Office (TERO), which may require certain fees be paid.

The Government is not subject to TERO requirements and is not a party to any agreements between the Tribe and Contractor pursuant to the TERO.

For further information on the TERO requirements, contact the [INSERT TRIBE NAME] TERO at:

[INSERT TRIBE NAME] Tribal Employment Rights Office

[INSERT CONTACT INFORMATION]

WFL Specification 01/01/14 1050130

Include the following in projects for Glacier National Park solicitations.

Materials obtained from within the boundaries of the Blackfeet Reservation may be subject to the Blackfeet Tribal Employment Rights Office (TERO), which may require certain fees be paid.

The Government is not subject to TERO requirements and is not a party to any agreements between the Tribe and Contractor pursuant to the TERO.

For further information on the TERO requirements, contact the Blackfeet TERO at:

Blackfeet Tribal Employment Rights Office

P.O. Box 850

Browning, Montana 59417

Phone: 406.330.7887

WFL Specification 04/02/21 1050140

Include the following when staging or stockpiling of materials is required.

Only insert “portions of the right-of-way approved by the CO” if there is a possibility of portions being approved.

Coordinate with Partner Agency and edit as required.

### 105.04 Handling and Storing Material.

Delete the text of the second paragraph and substitute the following:

Use only [INSERT AREA NAME OR LOCATION AND/OR portions of the right-of-way approved by the CO] for staging or storing of materials such as culverts, geotextile fabric, temporary traffic control devices; and for equipment parking.

Provide additional space as needed. Do not use private property for staging, storage, or disposal without written permission of the owner or lessee and prior to completion of the requirements of subsection 107.10(d). Submit copies of agreements and documents and do not use property until approved by CO.