## Section 106. — ACCEPTANCE OF WORK

01 JUL 2024– FP-24

WFL Specification 01 JUL 2024 1060010

Include the following in all projects.

### 106.01 Conformity with Contract Requirements.

Add the following to the second paragraph:

References to the MUTCD refer to the 2009 MUTCD with Revision Numbers 1, 2 and 3 incorporated.

Add the following:

Obtain copies of the following documents at:

<https://highways.dot.gov/federal-lands/construction/paynotes>

* *Construction Paynote Examples*, dated August 2011.

Obtain copies of the following documents at:

<https://highways.dot.gov/federal-lands/materials>

* *WFLHD Sampling and Testing Methods*;
* Materials Testing Forms;
* FLH T 521 – *Standard Method of Test for Determining Riprap Gradation by Wolman* Count; and
* FLH Addendum to AASHTO T 308 – *Standard Method of Test for Correction Factors for Hot Mix Asphalt (HMA) Containing Recycled Asphalt Pavement (RAP) by the Ignition Method*.

WFL Specification 01 APR 2024 1060020

Include the following on all projects.

### 106.03 Certification.

Add the following after the second paragraph:

Obtain required certifications and maintain records of all required certifications according to Subsections 103.04 and 153.04(a).

Submit a completed Form WFLHD 87 *Certification of Compliance* with each material requiring a certification. An electronic version may be found at:

<https://highways.dot.gov/federal-lands/construction/forms-wfl>

Submit all certifications to the CO unless otherwise specified in the Section ordering the work.