## Section 618. — CONCRETE BARRIERS

01 APR 2024 – FP-24

Construction Requirements

WFL Specification 01 APR 2024 6180001

Include the following when pinned concrete barrier is required to reduce deflection distance.

### 618.04 Concrete Barriers.

Add the following:

Pin concrete barrier as shown in the plans.