## Section 705. — ROCK

01 APR 2024 – FP-24

### 705.02 Rock for Riprap.

CAUTIONARY STATEMENT

Note:

When designing riprap structures within the limits of a water channel consider the effect of voids and water flow. Revise gradation requirements if necessary to choke the riprap to ensure water flows over rather than under the riprap.

Consult your COTR or Hydraulics and Materials Engineers.

Riprap may also requiring choking when covered by topsoil or aggregates.